;Description##OTHER##;Assembly Code##OTHER##;Dimensions##OTHER##;Montage##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Color of the light##OTHER##;Light Loss Factor##OTHER##;Driver##OTHER##;Voltage##ELECTRICAL_POTENTIAL##VOLTS;Voltage (range)##OTHER##;Body material##OTHER##;Colour##OTHER##;Diffuser##OTHER##;Lamp##OTHER##;Operating temperature range##OTHER##;Lifetime of LED sources##OTHER##;Lx/By##OTHER##;CRI##OTHER##;SDCM##OTHER##;Beam angle##OTHER##;Protection degree##OTHER##;Impact resistant##OTHER##;Protection against electric shock##OTHER##;Photobiological risk class (IEC/EN 62471)##OTHER##;Power factor##OTHER##;Length##LENGTH##MILLIMETERS;Width##LENGTH##MILLIMETERS;Height##LENGTH##MILLIMETERS;Diameter##LENGTH##MILLIMETERS;URL##OTHER##;Catalogue##OTHER##;Photometric Web File##OTHER##;Type Comments##OTHER##;Manufacturer##OTHER##
X-LINE SLIM RECESSED LED 4400 MICRO-PRM E 34 830 LINE-EL / L-1148MM;Recessed luminaires;19.3218.0020.34;1148 x 70 x 75;mounted in plasterboard ceilings;24.7;3275;133;3000;3000;0.7432;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 88,4° / 86°;IP40;IK04;I;-;0,9;1148;70;75;0;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/x-line-slim-recessed-led-line/;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/x-line-slim-recessed-led-line/19.3218.0020.34/;19.3218.0020.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM RECESSED LED 4400 MICRO-PRM E 34 830 LINE-S / L-1136MM;Recessed luminaires;19.3218.0021.34;1136 x 70 x 75;mounted in plasterboard ceilings;24.7;3275;133;3000;3000;0.7432;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 88,4° / 86°;IP40;IK04;I;-;0,9;1136;70;75;0;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/x-line-slim-recessed-led-line/;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/x-line-slim-recessed-led-line/19.3218.0021.34/;19.3218.0021.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM RECESSED LED 4400 MICRO-PRM E 34 830 LINE-EP / L-1148MM;Recessed luminaires;19.3218.0022.34;1148 x 70 x 75;mounted in plasterboard ceilings;24.7;3275;133;3000;3000;0.7432;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 88,4° / 86°;IP40;IK04;I;-;0,9;1148;70;75;0;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/x-line-slim-recessed-led-line/;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/x-line-slim-recessed-led-line/19.3218.0022.34/;19.3218.0022.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM RECESSED LED 4400 MICRO-PRM E 34 840 LINE-EL / L-1148MM;Recessed luminaires;19.3218.0023.34;1148 x 70 x 75;mounted in plasterboard ceilings;24.7;3393;137;4000;4000;0.7432;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 88,4° / 86°;IP40;IK04;I;-;0,9;1148;70;75;0;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/x-line-slim-recessed-led-line/;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/x-line-slim-recessed-led-line/19.3218.0023.34/;19.3218.0023.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM RECESSED LED 4400 MICRO-PRM E 34 840 LINE-S / L-1136MM;Recessed luminaires;19.3218.0024.34;1136 x 70 x 75;mounted in plasterboard ceilings;24.7;3393;137;4000;4000;0.7432;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 88,4° / 86°;IP40;IK04;I;-;0,9;1136;70;75;0;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/x-line-slim-recessed-led-line/;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/x-line-slim-recessed-led-line/19.3218.0024.34/;19.3218.0024.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM RECESSED LED 4400 MICRO-PRM E 34 840 LINE-EP / L-1148MM;Recessed luminaires;19.3218.0025.34;1148 x 70 x 75;mounted in plasterboard ceilings;24.7;3393;137;4000;4000;0.7432;standard on/off (E);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 88,4° / 86°;IP40;IK04;I;-;0,9;1148;70;75;0;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/x-line-slim-recessed-led-line/;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/x-line-slim-recessed-led-line/19.3218.0025.34/;19.3218.0025.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM RECESSED LED 4400 MICRO-PRM EDD 34 827-865 LINE-1EL / L-1148MM TUNABLE WHITE;Recessed luminaires;19.3218.0032.34;1148 x 70 x 75;mounted in plasterboard ceilings;32;3399;106;4000;2700 ÷ 6500;0.7432;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;50000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 88,4° / 86°;IP40;IK04;I;-;0,9;1148;70;75;0;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/x-line-slim-recessed-led-line/;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/x-line-slim-recessed-led-line/19.3218.0032.34/;19.3218.0032.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM RECESSED LED 4400 MICRO-PRM EDD 34 827-865 LINE-1S / L-1136MM TUNABLE WHITE;Recessed luminaires;19.3218.0033.34;1136 x 70 x 75;mounted in plasterboard ceilings;32;3399;106;4000;2700 ÷ 6500;0.7432;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;50000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 88,4° / 86°;IP40;IK04;I;-;0,9;1136;70;75;0;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/x-line-slim-recessed-led-line/;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/x-line-slim-recessed-led-line/19.3218.0033.34/;19.3218.0033.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM RECESSED LED 4400 MICRO-PRM EDD 34 827-865 LINE-1EP / L-1148MM TUNABLE WHITE;Recessed luminaires;19.3218.0034.34;1148 x 70 x 75;mounted in plasterboard ceilings;32;3399;106;4000;2700 ÷ 6500;0.7432;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;50000;L80/B10;>80;3;(C0-C180) / (C90-C270) - 88,4° / 86°;IP40;IK04;I;-;0,9;1148;70;75;0;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/x-line-slim-recessed-led-line/;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/x-line-slim-recessed-led-line/19.3218.0034.34/;19.3218.0034.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM RECESSED LED 4400 MICRO-PRM EDD 34 830 LINE-1EL / L-1148MM;Recessed luminaires;19.3218.0026.34;1148 x 70 x 75;mounted in plasterboard ceilings;24.7;3275;133;3000;3000;0.7432;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 88,4° / 86°;IP40;IK04;I;-;0,9;1148;70;75;0;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/x-line-slim-recessed-led-line/;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/x-line-slim-recessed-led-line/19.3218.0026.34/;19.3218.0026.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM RECESSED LED 4400 MICRO-PRM EDD 34 830 LINE-1S / L-1136MM;Recessed luminaires;19.3218.0027.34;1136 x 70 x 75;mounted in plasterboard ceilings;24.7;3275;133;3000;3000;0.7432;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 88,4° / 86°;IP40;IK04;I;-;0,9;1136;70;75;0;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/x-line-slim-recessed-led-line/;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/x-line-slim-recessed-led-line/19.3218.0027.34/;19.3218.0027.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM RECESSED LED 4400 MICRO-PRM EDD 34 830 LINE-1EP / L-1148MM;Recessed luminaires;19.3218.0028.34;1148 x 70 x 75;mounted in plasterboard ceilings;24.7;3275;133;3000;3000;0.7432;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 88,4° / 86°;IP40;IK04;I;-;0,9;1148;70;75;0;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/x-line-slim-recessed-led-line/;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/x-line-slim-recessed-led-line/19.3218.0028.34/;19.3218.0028.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM RECESSED LED 4400 MICRO-PRM EDD 34 840 LINE-1EL / L-1148MM;Recessed luminaires;19.3218.0029.34;1148 x 70 x 75;mounted in plasterboard ceilings;24.7;3393;137;4000;4000;0.7432;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 88,4° / 86°;IP40;IK04;I;-;0,9;1148;70;75;0;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/x-line-slim-recessed-led-line/;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/x-line-slim-recessed-led-line/19.3218.0029.34/;19.3218.0029.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM RECESSED LED 4400 MICRO-PRM EDD 34 840 LINE-1S / L-1136MM;Recessed luminaires;19.3218.0030.34;1136 x 70 x 75;mounted in plasterboard ceilings;24.7;3393;137;4000;4000;0.7432;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 88,4° / 86°;IP40;IK04;I;-;0,9;1136;70;75;0;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/x-line-slim-recessed-led-line/;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/x-line-slim-recessed-led-line/19.3218.0030.34/;19.3218.0030.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
X-LINE SLIM RECESSED LED 4400 MICRO-PRM EDD 34 840 LINE-1EP / L-1148MM;Recessed luminaires;19.3218.0031.34;1148 x 70 x 75;mounted in plasterboard ceilings;24.7;3393;137;4000;4000;0.7432;DIM DALI (EDD);230;220..240 V, 50..60 Hz;LUXIONA_Aluminum;LUXIONA_RAL 9016 (white);LUXIONA_Micro-PRM;LED;5 ÷ 30;100000 (1) / 147000 (2);L80/B10 (1) / L70/B10 (2);>80;3;(C0-C180) / (C90-C270) - 88,4° / 86°;IP40;IK04;I;-;0,9;1148;70;75;0;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/x-line-slim-recessed-led-line/;https://luxiona.pl/en/oferta/oprawy-do-wbudowania/x-line-slim-recessed-led-line/19.3218.0031.34/;19.3218.0031.34_LDT.ies;We reserve the right to make technical changes without  notice. Please contact your local sales office for further  information. ;LUXIONA
